**After decompression, launch the sample via OPC\_DEMO.exe.**



**In Serial mode (corresponds to OPC SERIAL HOST/SLAVE/EXT mode):** Select the corresponding serial port from the Port dropdown and then click "Open" to connect the serial port.

**In Socket mode (corresponds to OPC SOCKET SERVER mode):** In the Host field, enter the local IP address of the POS machine, and then click "Connect" to connect to the OPC.

1. Connect to the OPC application via Serial/Socket.
2. Select the desired TransType, enter the amount and other parameters, then click ‘Send’ to initiate the transaction.
3. Click 'Cancel' to cancel the currently executing transaction.

Serial port screenshot:



Socket screenshot：

